Userful multiplatform user manual

|  |  |
| --- | --- |
| Step1 | **Must Check your Server**  1: CPU must support 64bit and the Virtualization  2: The Server Video must be Support on userful 是说服务端的视频格式必须支持Userful吗？  3: More than 30G Disk is recommended.  4: Internet network is available for software update  5: Software cannot be installed by usb-dvdrom, shall be installed by SATA/IDE dvd rom  6: a switcher or router is required;  7: AMD CPU is not recommended. |
| Step2 | Step by step , Reboot    Set Administrator and Password: set root/111111    Set user and Password, set centerm/111111 |
| Step3 | **Update useful package should be performed with a root user, root account and password shall be required;**  **Installing external packages will take 10 mins or more**    **After installed, reboot, and login centerm/111111 user mode** |
| Step4 | **At user mode (centerm/111111)**  **Run “Control center”, input 111111( user password)** |
| Step5 | **The zero client centerm logo**    **The Server Search the Zero Client，and set zero client ip mode (dhcp or static)**  **Then, Assgin All** |
| Step6 | **Run virtual box, install xp , win7 or other OS** |
| Step7 | * **The userful multiplatform linux have some functions, the important functions is sharing linux and userful-virtual box vdi (need have virtual box vm os)**   **Create** **Profile**       * **Set Station Mapping to Profile (** drag 2/3/4 station id to prolife, canot drag ID1) ,Apply |
| Step8 | **The Zero client then first show userful logo, , and next show OS** |